# ITEM 102.533 TREE CARE - WATERING GALLON

The work under this item shall conform to the relevant provisions of Section 440 and 771 of the Standard Specifications and the following:

The purpose of this item is to provide watering for tree care during and after root pruning as directed by the Arborist. Watering shall occur during daytime hours only.

## MATERIAL

Water shall be water from an approved source.

## SUBMITTALS

Schedule for watering shall be determined in consultation with the arborist. Expected schedule shall be submitted to the Engineer. Source of the water shall be approved by the Engineer and included in the submittal.

Contractor shall submit metered record of water used or other measure approved by the Engineer. Record must show date of watering and quantity used.

## METHODS

At least one day prior to watering on site, the contractor shall notify the Engineer.

Watering equipment shall be approved by the Engineer prior to watering under this item. Equipment shall be such that there is no water leaking from the tank, hoses, or any other parts. Water shall be pumped and have a minimum flow of 95 PSI. Gravity fed watering shall not be accepted under this item.

If water runs off root zone area due to slope, too high a flow rate, slow infiltration, or any other reason, water will not be approved for payment.

Watering method shall not damage plants or seeded areas or cause erosion. All damages shall be repair at the Contractor’s expense.

## MEASUREMENT AND PAYMENT

Item 102.533 shall be measured by the Gallon and shall be based on the submittals described herein. Payment shall be for all labor, equipment, and materials to complete the work specified.

Item 102.533 will be paid for at the Contract unit price per Gallon which price shall include all labor equipment, materials and incidental costs required to complete the work.