# Item 698.31 Geotextile Fabric for Temporary Soil Protection SY

The work under this item shall include furnishing and placement of geotextile fabric for temporary soil protection as shown on the plans and/or as required by the Engineer. All work shall be done in conformance with the applicable sections of the Standard Specifications.

Geotextile Fabric for Temporary Soil protection shall conform to the requirements of AASHTO M 288 and shall be listed on the Qualified Construction Material’s List and be approved for Separation.

Six inches of crushed stone shall be placed over the fabric prior to placement of fill. Stone shall meet M2.01.1.

Following completion of construction work, fill, stone, and fabric shall be removed and properly disposed off-site or as required by the Engineer.

Item 698.31 will be measured and paid for at the Contract unit price bid per Square Yard, which prices shall include the fabric, all labor, tools, materials, stone, any necessary incidental items to provide complete in place installation, and removal and disposal of stone and fill. Overlapped matting will not be measured for payment.

Crushed stone and removal of stone will be incidental to this item.

Schedule of Payment shall be as follows:

* 50% upon approval of installation
* 50% upon removal of fabric and stone as required by the Engineer.