TO BE COMPLETED BY RESIDENT FOR HOME SAMPLING:

Address: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Town\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Phone No \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ (optional)

E-Mail \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_(optional)

Were there any recent changes to your home plumbing? [ ]  Yes [ ]  No

Describe the changes, including the date they were made: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Do you have a treatment system or filter? [ ]  Yes [ ]  POU [ ]  POE [ ]  No

Point of Use treatment Device (POU) /Point of Entry treatment Device (POE)

Indicate Location of Sample Collected for Lead & Copper Testing:

Please read the attached instructions. Collect cold water only from Kitchen Faucet (or Bathroom Faucet) where you would normally use the water to drink or prepare food. The water must stay stagnant (not used in the house) for at least 6 hours before sample collection.

Sample location:[ ]  Kitchen [ ]  Bathroom

Sample was taken: Time \_\_\_\_\_\_\_\_ Date \_\_\_\_\_\_\_\_

Water was last used before sample was taken: Time \_\_\_\_\_\_\_\_ Date \_\_\_\_\_\_\_\_

*I have read the attached Sample Collection Instructions and have taken a tap sample in accordance with these procedures:* [ ]  Yes [ ]  No

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_/\_\_\_\_/\_\_\_\_

# Resident’s Signature Date

============================================================================

TO BE COMPLETED BY PWS COLLECTOR AFTER VERIFYING THAT THE SAMPLE WAS COLLECTED CORRECTLY AND THAT THE COC WAS PROPERLY COMPLETED:

## Sample accepted: \_\_\_\_\_

## Sample rejected: \_\_\_\_\_ (check applicable reason)

## [ ]  Collected at wrong location

## [ ]  COC is not filled out properly

[ ]  Improper standing time

[ ]  Plumbing modification to interior piping or home service line

[ ]  Installation of treatment device (POU/POE) that removes inorganic contaminants

Note: If the sample is rejected, the collector shall indicate the reason on the COC and provide a copy to the homeowner/resident. The rejected sample must be discarded, and a new sample kit should be provided to the homeowner/resident within one week, if applicable.

*I certify under penalty of law that I am the person authorized to fill out this form and the information contained herein is true, accurate and complete to the best of my knowledge and belief.*

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_/\_\_\_\_/\_\_\_\_

PWS Collector’s Signature Print Name Date

============================================================================

PWS Filing Requirement

PWS must staple this completed form to the certified laboratory chain of custody form for this sample and keep copies of both documents in accordance with 310 CMR 22.00 record keeping requirements.

### INSTRUCTIONS FOR RESIDENTS FOR HOME SAMPLING

These samples are being collected to determine the contribution of faucet fixtures (kitchen or bathroom) and household pipes and/or solder to the lead and copper levels in tap water. This sampling effort is required by the Massachusetts Department of Environmental Protection and is being accomplished through the cooperation of homeowners and residents.

A sample is to be collected after an extended period (at least 6 hours) of stagnant water conditions (i.e. no water use during this period) within the interior piping. **Do not intentionally flush the line before the start of the 6-hour period, rather, use water normally.** Due to this requirement, either early mornings or evenings upon returning from work are the best times for collecting samples. The collection procedure is as follows:

1. Prior arrangements will be made with the homeowner/resident to coordinate sample collection. Dates will be set for sample kit delivery and pick-up by water department staff.
2. **Samples must be collected after a minimum of 6 hours without water use.** The water department recommends that either early morning or upon returning home are the best sampling times to ensure that the necessary stagnant water condition exists.
3. A wide-mouth bottle must be used to collect each one-liter (1000 mL) sample. Wide-mouth bottles offer advantages over narrow-mouth bottles because they allow for a higher flow rate during sample collection. A higher flow rate can result in greater release of particles and colloidal lead and therefore is more conservative in terms of identifying lead concentrations.
4. **A kitchen or bathroom cold-water faucet must be used for the sampling. Do not use a faucet with a treatment device or filter,** e.g., a filter/softener or other device treating all of the water entering your home (POE) or a device exclusively filtering water delivered to the kitchen faucet (POU). If you have such a device, then collect the sample from the bathroom. In the kitchen, sample collection from a single lever faucet or tempered faucet should be avoided, if possible. **Do not remove the aerator prior to sampling**. Place the open sample bottle under the faucet and open the cold-water tap. Fill the sample bottle to the line marked “1000-mL” and turn off the water.
5. Tightly cap the bottle and place in the sample kit provided. Please review the sample kit label at this time to ensure that all information contained in the label is correct. Complete the COC.
6. **Be sure to note on the label provided and on the COC if plumbing repairs or replacements have been done in the home since the previous sampling event. Also, if you have a treatment system or home filters, please inform the water department and indicate this on the COC.**
7. Place the sample kit outside the residence in the location where the kit was delivered in order that the water department may pickup the sample kit.
8. Results from this monitoring effort will be provided to participating customers when reports are generated for the State unless excessive lead and/or copper levels are found. In such cases, immediate notification will be provided.

Call \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ at \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_if you have any questions regarding these instructions.

For more information on Lead in Drinking Water, see <https://www.mass.gov/guides/is-there-lead-in-my-tap-water>

**Notes:**

* **If the sample is rejected, the collector shall indicate the reason on the COC and provide a copy to the homeowner. The collector must discard the sample and provide a new sample kit to the homeowner within one week, if applicable.**
* **Sampling results are a public record. Please remember that all records are required to be maintained for 12 years.**