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       Monthly UST Inspection Log

	Monthly UST Inspection Log
	Staple Relevant Documentation Here 

	Inspector Name: 
     
	Operator ID#: 
     
	Inspection Date/Time:
     

	Inspector Type:  |_|  Class A Operator      |_|  Class B Operator      |_|  Class A/B Operator    
 |_|  Inspector under direction of Owner, Operator, or Class A, B or A/B Operator   
                 Name of that Owner, Operator, or Class A, B, or A/B Operator:                                                                                                                       


	Inspection Item
	Result
	If “No,” explain why/describe corrective actions taken
	Date resolved

	1. Leak Detection
**If UST(s) utilize(s) continuous monitoring, attach the liquid status report to the top right corner.

	a. Is all leak detection equipment “on,” and operating as usual with no alarms?
	|_| Yes   |_| No
	
	

	b. Were all indications of leakage or release responded to in accordance with 310 CMR 80.26?
	|_| Yes   |_| No
|_| NA
	
	

	c. Are all leak detection records complete, accurate, and current?
	|_| Yes   |_| No
	
	

	2. Spill Buckets, Covers, and Sensors

	a. Are all spill buckets clean and free of solid and liquid material?
	|_| Yes   |_| No
	
	

	b. Are all spill buckets free from signs of corrosion, deterioration, cracks, and holes?
	|_| Yes   |_| No
	
	

	c. Are all spill bucket sensors positioned in accordance with manufacturer’s specifications?
	|_| Yes   |_| No

|_| NA
	


	

	d. If no manufacturer’s specifications exist, are the spill bucket sensors placed at the lowest possible location in the spill buckets?
	|_| Yes   |_| No
|_| NA
	
	

	e. Are all fill pipes free of obstructions and secured with a cap?
	|_| Yes   |_| No
	
	

	f. For double-walled spill buckets with interstitial monitoring, is the interstitial space free of liquids? 
	|_| Yes   |_| No
|_| NA
	
	

	3. Fill Cover Color-Coding

	a. Are all grade level fill covers color-coded in accordance with API RP 1637?
	|_| Yes   |_| No
	
	



Refer to 310 CMR 80.35 for a detailed description of the periodic inspection requirements, and 310 CMR 80.26 for specifics of testing and investigations required for different types of leak detection.  
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