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       UST Sump Periodic Inspection Log
	UST Sump Periodic Inspection Log
**Complete this log every 90 days for sumps not continuously monitored, and annually for sumps that are continuously monitored.

	Inspector Name: 
     
	Operator ID#: 
     
	Inspection Date/Time:
     

	Inspector Type:  |_|  Class A Operator      |_|  Class B Operator      |_|  Class A/B Operator                           

                            |_|  Inspector under direction of Owner, Operator, or Class A, B or A/B Operator   
                                    Name of that Owner, Operator, or Class A, B, or A/B Operator:                                                            


	Inspection Item
	Result
	If “No,” explain why/describe corrective actions taken
	Date resolved

	1. Are sumps, sump covers, and manhole covers free of damage, corrosion, and breakage and wear?
	|_| Yes   |_| No
	
	

	2. Are sumps free of leaks to the containment areas and releases to the environment?
	|_| Yes   |_| No
	
	

	3. Are sumps clean and free of solid and liquid material?
	|_| Yes   |_| No
	
	

	4. For double-walled sumps, is the interstitial area free of liquid?
	|_| Yes   |_| No

 |_| NA
	
	

	5. Are all sump sensors operating in accordance with the manufacturer’s specifications?
	|_| Yes   |_| No

 |_| NA
	
	

	6. If no manufacturer’s specifications exist, are the sump sensors placed at the lowest possible location in the sumps?
	|_| Yes   |_| No

 |_| NA
	
	

	7. If sump sensors have been or are in alarm, have the alarms been addressed?
	|_| Yes   |_| No

 |_| NA
	
	


Refer to 310 CMR 80.35 for a detailed description of the periodic inspection requirements.
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