*Attention Public Water Systems: Please adapt this form for your own use. Replace green sections as indicated. An electronic copy of this form is located at the MassDEP website at* [*https://www.mass.gov/lists/lead-copper-forms-templates*](https://www.mass.gov/lists/lead-copper-forms-templates)

# 含铅供水管道更换计划

市/镇：[City/Town]

PWS名称：[PWS Name]

PWS ID#：[PWS ID#]

# 铅检测结果高于行动水平

日期：[DATE]

地址：[Address]

姓名：[Name] 电话号码：[Phone Number]

尊敬的业主：

如你所知，[DATE the portion of lead service line owned by city/town was replaced]，我们更换了市/镇负责的含铅供水管道部分，并于 [DATE PWS took a water sample within the lead service line to test for lead level after the replacement]在含铅供水管道内采集了水样，以检测更换后的铅水平。

您部分更换的含铅供水管道中的铅含量结果为[lead result in water at homeowner’s partially replaced lead service line, in ppm]ppm，高于《铅铜规则》规定的铅行动水平0.015 ppm。

正如我们在“含铅供水管道更换计划”的第一份和第二份通知中告知您的那样，您选择不更换的那部分含铅供水管道仍然是铅的来源，如果水不使用的时间超过六小时，铅就会浸出。实际上，部分更换可能会暂时增加铅含量。

市/镇和 [PWS Name] PWS 建议采取以下措施，以防饮用水中可能存在铅：

* **最重要的是——**水龙头放水，直到水感觉很冷后才使用。街道水管里的水不含铅。
* 水龙头的热水切勿饮用或烹饪，特别是勿用于制作婴儿配方奶。
* 切勿煮沸水以除去铅。长时间的煮沸水可能会使铅浓度更高，并且
* 替换您负责的含铅供水管道的剩余部分。

如果您对饮用水中的铅或铅抽样结果有任何疑问，请随时联系 [NAME of individual to contact with questions regarding lead in drinking water or the lead sampling result]，联系方式[contact PHONE number or EMAIL address] 或*水务主管*，联系方式 [Water Superintendent contact PHONE or EMAIL address]。

[Name and signature of either Town Manager or DPW Director]

镇长 DPW主任