*Attention Public Water Systems: Please adapt this form for your own use. Replace green sections as indicated. An electronic copy of this form is located at the MassDEP website at* [*https://www.mass.gov/lists/lead-copper-forms-templates*](https://www.mass.gov/lists/lead-copper-forms-templates)

# 含鉛供水管道更換計畫

市/鎮：[City/Town]

PWS名稱：[PWS Name]

PWS ID#：[PWS ID#]

# 鉛檢測結果高於行動水準

日期：[DATE]

地址：[Address]

姓名：[Name] 電話號碼：[Phone Number]

尊敬的業主：

如你所知，[DATE the portion of lead service line owned by city/town was replaced]，我們更換了市/鎮負責的含鉛供水管道部分，並於 [DATE PWS took a water sample within the lead service line to test for lead level after the replacement]在含鉛供水管道內採集了水樣，以檢測更換後的鉛水準。

您部分更換的含鉛供水管道中的鉛含量結果為 [lead result in water at homeowner’s partially replaced lead service line, in ppm] ppm，高於《鉛銅規則》規定的鉛行動水準0.015 ppm。

正如我們在“含鉛供水管道更換計畫”的第一份和第二份通知中告知您的那樣，您選擇不更換的那部分含鉛供水管道仍然是鉛的來源，如果水不使用的時間超過六小時，鉛就會浸出。實際上，部分更換可能會暫時增加鉛含量。

市/鎮和 [PWS Name] PWS 建議採取以下措施，以防飲用水中可能存在鉛：

* **最重要的是——**水龍頭放水，直到水感覺很冷後才使用。街道水管裡的水不含鉛。
* 水龍頭的熱水切勿飲用或烹飪，特別是勿用於製作嬰兒配方奶。
* 切勿煮沸水以除去鉛。長時間的煮沸水可能會使鉛濃度更高，並且
* 替換您負責的含鉛供水管道的剩餘部分。

如果您對飲用水中的鉛或鉛抽樣結果有任何疑問，請隨時聯繫 [NAME of individual to contact with questions regarding lead in drinking water or the lead sampling result]，聯繫方式 [contact PHONE number or EMAIL address] 或*水務主管*，聯繫方式 [Water Superintendent contact PHONE or EMAIL address]。

[Name and signature of either Town Manager or DPW Director]

鎮長 DPW主任