{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Groundwater Table"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Groundwater Table","index":0,"n_rows":13,"n_cols":25,"rows_kept":13,"cut":false,"hidden":false,"merged":[[11,0,11,19],[2,0,3,0],[0,2,0,24],[8,0,9,0],[0,0,1,0],[0,1,1,1],[6,0,7,0],[4,0,5,0]]}
["Sample \ncollected      \nweek of","Reported by1 ","Tritium concentration p(Ci/L)"]
[null,null,"MW-201","MW-202S","MW-202I","MW-204 ","MW-205","MW-206 ","MW-207","MW-208S","MW-208I","MW-209","MW-210","MW-211","MW-212","MW-213","MW-214"," MW-215 ","MW-216","MW-217","MW-218","MW-219","MW-220","MW-3","MW-4 R"]
["2022-08-01","HOLTEC-TEL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"<566"]
["2019-02-26","MDPH-MERL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"<300"]
["2022-08-15","HOLTEC-TEL","<524","<528","<523","<582","<604",null,"<618","<593","<598","<558","<599","<527",null,"<599",null,"<577",null,"<596","<547",null,"<550",null,"<616"]
["2019-02-26","MDPH-MERL",354.7,"<300","<300","<300","<300",null,"<300","<300",305.60000000000002,"<300","<300","<300",null,307.5,null,"<300",null,"<300",303.8,null,"<300",null,"<300"]
["2022-08-22","HOLTEC-TEL",null,null,null,null,null,"<627",null,null,null,null,null,null,"<617",null,"<633",null,"<625",null,null,"<636"]
["2019-02-26","MDPH-MERL",null,null,null,null,null,"<300",null,null,null,null,null,null,"<300",null,"<300",null,396.4,null,null,"<300"]
["2022-12-05","HOLTEC-TEL","<555","<582","<544","<532","<563","<534","<558","<502","<561","<540","<577","<575","<518","<578","<557","<618",965,"<506","<588","<562","<548","<558","<623"]
[null,"MDPH-MERL","<300","<300","<300","<300","<300","<300","<300","<300","<300","<300","<300","<300","<300","<300","<300","<300",538.6,"<300","<300","<300","<300","<300","<300"]
[]
["1. Sample analysis for Holtec is by Teledyne and for MDPH is by the Massachusetts Environmental Radiation Laboratory (MERL). "]
["\"<\" Results are less than the detection limit shown. MERL's lower detection limit is 300 p(Ci/L)."]